|  |  |
| --- | --- |
| Sum of two numbers (with procedure)*Demo program*print macro args mov dx,offset args mov ax,0900h int 21h endmdata segmentmsg1 db 0dh,0ah,"Enter first No.:$"msg2 db 0dh,0ah,"Enter second No.:$"msg3 db 0dh,0ah,"Sum is:$"n1 dw ?outs dw 10 dup(?)data ends | code segmentassume cs:code,ds:datastart: mov ax,data mov ds,ax print msg1 call read mov n1,cx print msg2 call read mov ax,n1 add ax,cx call disp print msg3 print outs mov ax,4c00h int 21hReadDisplaycode endsend start |