|  |  |
| --- | --- |
| Sum of two numbers (with procedure)  *Demo program*  print macro args  mov dx,offset args  mov ax,0900h  int 21h  endm  data segment  msg1 db 0dh,0ah,"Enter first No.:$"  msg2 db 0dh,0ah,"Enter second No.:$"  msg3 db 0dh,0ah,"Sum is:$"  n1 dw ?  outs dw 10 dup(?)  data ends | code segment  assume cs:code,ds:data  start: mov ax,data  mov ds,ax  print msg1  call read  mov n1,cx  print msg2  call read  mov ax,n1  add ax,cx  call disp  print msg3  print outs  mov ax,4c00h  int 21h  Read  Display  code ends  end start |